{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":65,"n_cols":8,"rows_kept":65,"merged":[[2,0,2,7],[3,0,3,7],[16,7,17,7],[21,7,23,7],[24,7,25,7],[52,7,55,7]],"flags":["formulas_cached_only"]}
["附件1"]
[]
["2021-2023年江苏省中央财政农机购置补贴机具补贴额一览表"]
["（第二批）"]
[]
["序号","大类","小类","品目","分档名称","基本配置和参数","中央财政\n补贴限额\n（元）","备注"]
[1,"耕整地机械","耕地机械","深松机","4—5铲凿铲式深松机","深松部件4、5个；深松铲结构型式：凿铲式；铲间距≥180mm",1680,"通用类"]
[2,"耕整地机械","耕地机械","深松机","6铲及以上凿铲式深松机","深松部件6个及以上；深松铲结构型式：凿铲式；铲间距≥180mm",1700,"通用类"]
[3,"耕整地机械","耕地机械","深松机","4—5铲偏柱式、全方位式深松机","深松部件4、5个；深松铲结构型式：偏柱式或全方位式；铲间距≥330mm",2230,"通用类"]
[4,"耕整地机械","耕地机械","深松机","6铲及以上偏柱式、全方位式深松机","深松部件6个及以上；深松铲结构型式：偏柱式或全方位式；铲间距≥330mm",2900,"通用类"]
[5,"种植施肥机械","播种机械","免耕播种机","7—11行免耕条播机","7行≤播种行数≤11行",2250,"通用类"]
[6,"种植施肥机械","播种机械","免耕播种机","12—18行免耕条播机","12行≤播种行数≤18行",2500,"通用类"]
[7,"种植施肥机械","播种机械","免耕播种机","19—24行免耕条播机","19行≤播种行数≤24行",4000,"通用类"]
[8,"种植施肥机械","播种机械","免耕播种机","25行及以上免耕条播机","播种行数≥25行",4300,"通用类"]
[9,"种植施肥机械","播种机械","免耕播种机","4—5行免耕穴播机","普通排种器；播种行数4、5行",1200,"通用类"]
[10,"种植施肥机械","播种机械","免耕播种机","6行及以上免耕穴播机","普通排种器；播种行数≥6行",1200,"通用类"]
[11,"种植施肥机械","播种机械","免耕播种机","4—5行免耕精量播种机","精量排种器；播种行数4、5行",1400,"通用类。\n精量排种器包括气力式和达到精量要求的指夹式，其他列为普通型式。"]
[12,"种植施肥机械","播种机械","免耕播种机","6行及以上免耕精量播种机","精量排种器；播种行数≥6行",3100]
[13,"种植施肥机械","施肥机械","撒肥机","0.2—0.5m³悬挂式固态肥抛撒机","0.2m³≤料厢（肥箱）容积＜0.5m³；抛撒宽度≥5m",180,"非通用类"]
[14,"种植施肥机械","施肥机械","撒肥机","0.5—1m³悬挂式固态肥抛撒机","0.5m³≤料厢（肥箱）容积＜1m³；抛撒宽度≥5m",450,"非通用类"]
[15,"种植施肥机械","施肥机械","撒肥机","1m³及以上悬挂式固态肥抛撒机","料厢（肥箱）容积≥1m³；抛撒宽度≥5m",900,"非通用类"]
[16,"田间管理机械","植保机械","植保无人驾驶航空器","10—20L多旋翼植保无人驾驶航空器","10L≤药液箱额定容量＜20L；多旋翼；电动、油动、油电混动；电动须配置智能电池系统，含智能电池2组及以上；具有避障系统；具有RTK的高精度卫星导航定位系统；具有电子围栏",6000,"通用类。\n1.多旋翼植保无人驾驶航空器是由两个以上旋翼（含两个）组成，并通过多个旋翼在空气中旋转产生升力和拉力实现飞行并进行施药作业的无人飞机。\n2.智能电池系统由智能电池和智能电池充电器组成，具备过充保护、过放保护、短路保护和充放"]
[17,"田间管理机械","植保机械","植保无人驾驶航空器","20—30L多旋翼植保无人驾驶航空器","20L≤药液箱额定容量＜30L；多旋翼；电动、油动、油电混动；电动须配置智能电池系统，含智能电池2组及以上；具有避障系统；具有RTK的高精度卫星导航定位系统；具有电子围栏",9000]
[18,"田间管理机械","植保机械","植保无人驾驶航空器","30L及以上多旋翼植保无人驾驶航空器","药液箱额定容量≥30L；多旋翼；电动、油动、油电混动；电动须配置智能电池系统，含智能电池2组及以上；具有避障系统；具有RTK的高精度卫星导航定位系统；具有电子围栏",12000]
[19,"田间管理机械","植保机械","植保无人驾驶航空器","15L—25L单旋翼植保无人驾驶航空器","15L≤药液箱额定容量＜25L；单旋翼；电动、油动、油电混动；电动须配置智能电池系统，含智能电池2组及以上；具有避障系统；具有RTK的高精度卫星导航定位系统；具有电子围栏",6000,"电使用次数显示等功能。\n3.避障系统是指通过雷达或多目视觉等传感器主动检测障碍物并能实时归避的系统，通常有前避障、前后避障或绕障，不含使用航线规划绕障。"]
[20,"田间管理机械","植保机械","植保无人驾驶航空器","25L及以上单旋翼植保无人驾驶航空器","药液箱额定容量≥25L；单旋翼；电动、油动、油电混动；电动须配置智能电池系统，含智能电池2组及以上；具有避障系统；具有RTK的高精度卫星导航定位系统；具有电子围栏",6000]
[21,"收获机械","玉米收获机械","自走式玉米籽粒联合收获机","4行自走式玉米籽粒联合收获机","4行割台；2.2m≤工作幅宽＜2.8m；型式：自走式",28000,"通用类"]
[22,"收获机械","玉米收获机械","自走式玉米籽粒联合收获机","5行及以上自走式玉米籽粒联合收获机","5行及以上割台；工作幅宽≥2.8m；型式：自走式",42000,"通用类"]
[23,"收获机械","饲料作物收获机械","打（压）捆机","压缩室截面积（宽×高）0.102m2及以上方捆捡拾压捆机","方捆；压缩室截面积（宽×高）≥0.102m2；打结器数量≥2个；捡拾宽度≥0.7m",4200,"通用类"]
[24,"收获机械","饲料作物收获机械","打（压）捆机","压缩室截面积（宽×高）0.1344m2及以上方捆捡拾压捆机","方捆；压缩室截面积（宽×高）≥0.1344m2；打结器数量≥2个；捡拾宽度≥1.2m",10200,"通用类"]
[25,"收获机械","饲料作物收获机械","打（压）捆机","压缩室截面积（宽×高）0.154m2及以上方捆捡拾压捆机","方捆；压缩室截面积（宽×高）≥0.154m2；打结器数量≥2个；捡拾宽度≥1.7m",15000,"通用类"]
[26,"收获机械","饲料作物收获机械","打（压）捆机","压缩室截面积（宽×高）0.162m2及以上方捆捡拾压捆机","方捆；压缩室截面积（宽×高）≥0.162m2；打结器数量≥2个；捡拾宽度≥2.2m",16300,"通用类"]
[27,"收获机械","饲料作物收获机械","打（压）捆机","压缩室截面积（宽×高）0.1998m2及以上方捆捡拾压捆机（3个及以上打结器）","方捆；压缩室截面积（宽×高）≥0.1998m2；打结器数量≥3个；捡拾宽度≥2.2m",20000,"通用类"]
[28,"收获机械","饲料作物收获机械","打（压）捆机","压缩室直径0.5m及以上圆捆捡拾压捆机","圆捆；压缩室直径≥0.5m；压缩室宽度≥0.7m；捡拾宽度≥0.7m",4200,"通用类"]
[29,"收获机械","饲料作物收获机械","打（压）捆机","压缩室直径0.8m及以上圆捆捡拾压捆机","圆捆；压缩室直径≥0.8m；压缩室宽度≥0.8m；捡拾宽度≥1.2m",11400,"通用类"]
[30,"收获机械","饲料作物收获机械","打（压）捆机","压缩室直径1m及以上圆捆捡拾压捆机","圆捆；压缩室直径≥1m；压缩室宽度≥1m；捡拾宽度≥1.7m",12000,"通用类"]
[31,"收获机械","饲料作物收获机械","打（压）捆机","压缩室直径1.2m及以上圆捆捡拾压捆机","圆捆；压缩室直径≥1.2m；压缩室宽度≥1.2m；捡拾宽度≥2.2m",18300,"通用类"]
[32,"收获机械","饲料作物收获机械","打（压）捆机","压缩室截面积（宽×高）0.105m2及以上方捆压捆机","方捆；压缩室截面积（宽×高）≥0.105m2；功率≥15kW",5100,"通用类"]
[33,"收获机械","饲料作物收获机械","青饲料收获机","2—2.6m自走圆盘式青饲料收获机，带对辊式籽粒破碎机构","自走圆盘式；2m≤割幅＜2.6m；籽粒破碎机构：对辊式；配套发动机功率≥115kW",58700,"通用类"]
[34,"收获机械","饲料作物收获机械","青饲料收获机","2.6m及以上自走圆盘式青饲料收获机，带对辊式籽粒破碎机构","自走圆盘式；割幅≥2.6m；籽粒破碎机构：对辊式；配套发动机功率≥150kW",100000,"通用类"]
[35,"收获后处理机械","干燥机械","果蔬烘干机","容积20—40m³厢式果蔬烘干机","20m³≤有效烘干容积＜40m³；结构型式：厢式；热源装置：非燃煤型、非电加热炉型",3000,"非通用类"]
[36,"收获后处理机械","干燥机械","果蔬烘干机","容积40m³及以上厢式果蔬烘干机","有效烘干容积≥40m³；结构型式：厢式；热源装置：非燃煤型、非电加热炉型",4500,"非通用类"]
[37,"收获后处理机械","干燥机械","果蔬烘干机","容积20—40m³热泵型厢式果蔬烘干机","20m³≤有效烘干容积＜40m³；结构型式：厢式；热源装置：热泵；热泵额定功率（不含电辅助加热）≥4.5kW",7500,"非通用类"]
[38,"收获后处理机械","干燥机械","果蔬烘干机","容积40m³及以上热泵型厢式果蔬烘干机","有效烘干容积≥40m³；结构型式：厢式；热源装置：热泵；热泵额定功率（不含电辅助加热）≥9kW",9500,"非通用类"]
[39,"畜牧机械","畜产品采集加工机械设备","挤奶机","40杯组及以上鱼骨式挤奶机","杯组数≥40；型式：鱼骨式；脉动器型式：电子；计量方式：电子计量；脱杯方式：自动",84200,"通用类"]
[40,"畜牧机械","畜产品采集加工机械设备","挤奶机","20杯组及以上并列（转盘）式挤奶机","杯组数≥20；型式：并列（转盘）式；脉动器型式：电子；计量方式：电子计量；脱杯方式：自动",100000,"通用类"]
[41,"畜牧机械","畜产品采集加工机械设备","挤奶机","自动挤奶设备","套杯时间≤120s",120000,"通用类"]
[42,"畜牧机械","畜产品采集加工机械设备","贮奶（冷藏）罐","1000—3000L全自动清洗冷藏罐","1000L≤容量＜3000L；清洗方式：全自动清洗",3800,"通用类"]
[43,"畜牧机械","畜产品采集加工机械设备","贮奶（冷藏）罐","3000—6000L全自动清洗冷藏罐","3000L≤容量＜6000L；清洗方式：全自动清洗",8200,"通用类"]
[44,"畜牧机械","畜产品采集加工机械设备","贮奶（冷藏）罐","6000L及以上全自动清洗冷藏罐","容量≥6000L；清洗方式：全自动清洗",16430,"通用类"]
[45,"畜牧机械","畜产品采集加工机械设备","贮奶（冷藏）罐","速冷设备","额定生产率≥1500L/h",50000,"通用类"]
[46,"农业废弃物利用处理设备","废弃物处理设备","有机废弃物好氧发酵翻堆机","2.5—3m油动有机废弃物好氧发酵翻堆机","2.5m≤工作幅宽＜3m；配套动力型式：柴油机；配套总功率≥51.5kW",15000,"非通用类"]
[47,"动力机械","拖拉机","履带式拖拉机","50—70马力差速转向履带式拖拉机","50马力≤功率＜70马力；驱动方式：履带式；转向型式：差速式转向；最大牵引功率≥70%发动机标定功率；最小使用比质量≥35kg/kW",21200,"通用类。\n差速式转向是指用于液压机械双功率流驱动差速转向机构，实现履带车辆转向的差速式转向系统。"]
[48,"动力机械","拖拉机","履带式拖拉机","70—90马力差速转向履带式拖拉机","70马力≤功率＜90马力；驱动方式：履带式； 转向型式：差速式转向；最大牵引功率≥70%发动机标定功率；最小使用比质量≥35kg/kW",23800]
[49,"动力机械","拖拉机","履带式拖拉机","90—110马力差速转向履带式拖拉机","90马力≤功率＜110马力；驱动方式：履带式；转向型式：差速式转向；最大牵引功率≥70%发动机标定功率；最小使用比质量≥35kg/kW",31500]
[50,"动力机械","拖拉机","履带式拖拉机","110马力及以上差速转向履带式拖拉机","110马力≤功率；驱动方式：履带式；转向型式：差速式转向；最大牵引功率≥70%发动机标定功率；最小使用比质量≥45kg/kW",31500]
[51,"动力机械","拖拉机","履带式拖拉机","50—70马力轻型履带式拖拉机","50马力≤功率＜70马力；驱动方式：履带式；橡胶履带",14400,"通用类"]
[52,"动力机械","拖拉机","履带式拖拉机","70—100马力轻型履带式拖拉机","70马力≤功率≤100马力；驱动方式：履带式；橡胶履带",14400,"通用类"]
[53,"其他机械","其他机械","畜禽粪便发酵处理机","5—10m³罐式畜禽粪便发酵处理机","罐式；5m³≤盛料容器容积＜10m³",16000,"非通用类"]
[54,"其他机械","其他机械","畜禽粪便发酵处理机","10—30m³罐式畜禽粪便发酵处理机","罐式；10m³≤盛料容器容积＜30m³",30000,"非通用类"]
[55,"其他机械","其他机械","畜禽粪便发酵处理机","30—50m³罐式畜禽粪便发酵处理机","罐式；30m³≤盛料容器容积＜50m³",60000,"非通用类"]
[56,"其他机械","其他机械","沼气发电机组","50—100kW沼气发电机组","50kW≤额定功率＜100kW；气缸数≥4",22000,"非通用类"]
[57,"其他机械","其他机械","沼气发电机组","100—150kW沼气发电机组","100kW≤额定功率＜150kW；气缸数≥6",30000,"非通用类"]
[58,"其他机械","其他机械","沼气发电机组","150—200kW沼气发电机组","150kW≤额定功率＜200kW；气缸数≥8",38000,"非通用类"]
[59,"其他机械","其他机械","沼气发电机组","200kW及以上沼气发电机组","额定功率≥200kW；气缸数≥12",46000,"非通用类"]